\documentclass[11pt]{article}
\input{jmpstyle.tex}

\begin{document}
\JMPTitle{Paper 037 / Application 014}{StructureForge}{Autonomous In-Space Assembly and Industrialization}{June 13, 2026}{v0.1}{in-space assembly, orbital factories, autonomous robotics, ISRU, construction algebra, HTS infrastructure, directed-energy logistics, space industry, galactic civilization}

\begin{abstract}
A galactic civilization cannot launch its bones from Earth. It must learn to grow structure where structure is needed. \textit{StructureForge} is a proposed architecture for autonomous in-space assembly and industrialization: robotic yards, standard interfaces, digital twins, process certification, orbital warehouses, lunar extraction nodes, autonomous inspection, and self-expanding industrial grammars. The grounded claim is that in-space servicing, assembly, and manufacturing must be treated as an auditable production system with typed parts, typed processes, robotic guilds, fault ledgers, and local assurance. The speculative claim is that the mature off-world factory becomes a constructor algebra: a machine society that writes new machines into matter while preserving formal evidence that the construction is safe. This paper defines capability closure, forge graphs, assembly policies, risk-priced autonomy, and a phased route from ground demonstrators to orbital hubs, lunar foundries, asteroid foundries, and directed-energy logistics. The practical spine is fission/fusion baseload power, cryogenic and high-current superconducting infrastructure, quantum gravimetry for resource maps and construction metrology, and directed-energy sails for high-energy supply chains.
\end{abstract}

\tableofcontents
\clearpage

\section{01 / Problem}

The first space age was heroic logistics. Humans learned to place exquisitely engineered artifacts into orbit and keep a few of them alive. The next age cannot be heroic logistics. A galactic civilization requires industrial recursion: factories that build more factories, yards that assemble kilometer-scale structures, robots that inspect and repair each other, resource chains that turn regolith and metal-rich bodies into power, shielding, habitats, optics, propellant, and computational substrate.

Earth launch is a miraculous bottleneck. It can seed civilization, but it cannot be civilization. If every radiator, truss, mirror, pressure vessel, shield tile, power cable, antenna, cryogenic line, magnetic loop, and habitat rib must climb out of Earth's gravity well, then the architecture remains colonial cargo rather than local life.

Recent work in autonomous orbital inspection, mobile maintenance robots, in-orbit factories, and reinforcement-learning free-flyer tests points toward the right direction \cite{WangPostDeremetz2025,ChapinEtAl2025APIARY,LeutertEtAl2024Factory}. The missing piece is an operating and assurance architecture that makes autonomous construction legible enough to trust.

\begin{claim}[Industrial recursion claim]
A space civilization begins when off-world infrastructure produces more mission capability than it consumes from Earth over a bounded planning horizon.
\end{claim}

\section{02 / Model}

StructureForge models off-world industrialization as a typed transformation system. Let
\begin{equation}
    \mathcal{F}=\langle \mathcal{P},\mathcal{M},\mathcal{R},\mathcal{A},\mathcal{E},\mathcal{Q}\rangle,
\end{equation}
where $\mathcal{P}$ is the part library, $\mathcal{M}$ the material catalog, $\mathcal{R}$ the robot population, $\mathcal{A}$ the assembly actions, $\mathcal{E}$ the environment model, and $\mathcal{Q}$ the assurance system.

\begin{definition}[Forge graph]
A forge graph is a directed typed hypergraph
\begin{equation}
    \mathcal{G}_F=(V_{\mathrm{stock}},V_{\mathrm{parts}},V_{\mathrm{tools}},V_{\mathrm{products}},H_{\mathrm{process}},\tau),
\end{equation}
where a hyperedge consumes stocks, parts, tools, energy, time, and assurance evidence to produce new parts, repaired tools, waste streams, or mission products. The type map $\tau$ records geometry, material, interface, load path, environment rating, and certification state.
\end{definition}

\begin{definition}[Capability closure ratio]
For a planning horizon $T$, define
\begin{equation}
    \rho_F(T)=\frac{\mathrm{value}\left(\mathrm{capability\ produced\ and\ qualified\ off\ world\ over\ }T\right)}{\mathrm{value}\left(\mathrm{capability\ launched\ from\ Earth\ over\ }T\right)+\eta}.
\end{equation}
The industrial phase transition begins when $\rho_F(T)>1$ for a nontrivial capability family: truss, shielding, tanks, mirrors, radiators, antennas, propellant, habitats, or robotic repair.
\end{definition}

The assembly planner solves a risk-priced policy problem:
\begin{equation}
\begin{aligned}
    \pi^* = \arg\min_{\pi\in\Pi} \; \E\sum_{k=0}^{H} [&\alpha \Delta v_k + \beta E_k + \gamma t_k + \delta m_{\mathrm{consumed},k} \\
    &+ \lambda R_k - \mu V_{\mathrm{qualified},k}] \\
    \mathrm{s.t.}\quad & s_{k+1}=F(s_k,a_k,w_k),\quad a_k=\pi(o_{\leq k}),\\
    & \Pr[\mathrm{catastrophic\ interaction}]\leq \epsilon,\\
    & q_{\mathrm{evidence}}(p_k)\geq q_{\min}.
\end{aligned}
\label{eq:forgepolicy}
\end{equation}

\section{03 / Architecture}

\subsection{Typed matter}
The first principle is that matter must become programmable without becoming abstract. Every structural element carries a digital passport:
\begin{itemize}
    \item geometry and tolerance;
    \item material history;
    \item radiation and thermal exposure;
    \item load history;
    \item interface standard;
    \item inspection records;
    \item allowed transformations;
    \item retirement and recycling path.
\end{itemize}

\subsection{Robotic guilds}
StructureForge does not assume a single omnipotent robot. It defines guilds:
\begin{longtable}{p{0.25\linewidth}p{0.65\linewidth}}
\toprule
\textbf{Guild} & \textbf{Function}\\
\midrule
Surveyors & Map geometry, thermal state, radiation, dust, inventory, and hazards.\\
Handlers & Move parts, dock modules, stabilize loads, manage tethers, and perform logistics.\\
Joiners & Weld, bolt, latch, bond, weave, sinter, print, clamp, and tension.\\
Inspectors & Perform metrology, non-destructive testing, thermal inspection, and digital passport updates.\\
Healers & Repair cracks, replace nodes, re-route power, apply patches, and isolate damage.\\
Miners & Excavate, sort, crush, heat, chemically process, and feed stock to yards.\\
Teachers & Turn human-reviewed corrections into verified policies, simulations, and training curricula.\\
\bottomrule
\end{longtable}

\subsection{Standard interfaces}
Industrial recursion requires ruthless interface discipline. The standard interface family should include mechanical capture, power, thermal, data, fluids, structural load paths, fiducials, and repair access. A part that cannot be inspected or repaired by the local robot population is not civilization-grade.

\subsection{Digital process twin}
Every production run occurs in two places: matter and model. The digital twin tracks geometry, control decisions, environment, tolerances, anomalies, and evidence. It must be adversarial: if the real process diverges from the twin, the twin must lose confidence rather than silently absorb contradiction.

\begin{equation}
    \mathcal{L}_{\mathrm{twin}} = \sum_t \left\| y_t - h(\hat{s}_t) \right\|_{\Sigma_t^{-1}}^2 + \lambda_c C_{\mathrm{constraint}}(\hat{s}_t) + \lambda_a A_{\mathrm{unexplained}}(t).
\end{equation}

\subsection{Local assurance}
The site architecture for JMP0X1B requires claims and evidence to be auditable \cite{JMPIndex2026,JMPResearchPack2026}. StructureForge adopts the same principle for manufactured parts. A truss segment is not accepted because a robot says it is complete. It is accepted because its evidence package satisfies the relevant assurance compiler.

\section{04 / The non-negotiable practical spine}

\spinetable

In StructureForge, the spine becomes industrial rather than merely supportive.

\begin{itemize}
    \item \textbf{Directed-energy sails} are not just probes; they are supply-chain primitives. Beam arrays can deliver gram-to-kilogram precision cargo, momentum packets, emergency spares, and courier nodes. A mature beam array is both launcher and lighthouse.
    \item \textbf{HTS magnetic infrastructure} turns factories into electromagnetic organisms: mass drivers, magnetic bearings, plasma torches, high-current induction heating, magnetic dust traps, radiation shields, and superconducting energy storage.
    \item \textbf{Cryogenic power buses} allow large yards to route current safely through modular cold corridors, with quench-aware isolation inherited from the CryoBus direction \cite{JMPCryoBus2026}.
    \item \textbf{Quantum gravimetry} maps buried ice, lava tubes, voids, ore gradients, subsurface hazards, and mass distribution of large structures \cite{PhillipsEtAl2022}.
    \item \textbf{Fission/fusion power} supplies dark-site baseload, industrial heat, high-duty robotics, propellant plants, and eventually high-field experiments. Lunar ISRU fission co-generation concepts already point to direct coupling between reactor heat and industrial chemistry \cite{MerczReissReiter2025}.
\end{itemize}

\section{05 / Claims}

\begin{claim}[Typed interface supremacy]
Autonomy scales only when mechanical, electrical, thermal, fluidic, and data interfaces are typed tightly enough for robots to reason about them.
\end{claim}

\begin{claim}[Assurance bottleneck]
For in-space industrialization, verification and evidence packaging will be as limiting as robotic dexterity.
\end{claim}

\begin{claim}[Bootstrap threshold]
A settlement becomes industrial when its local forge graph contains at least one positive feedback cycle that increases qualified production capacity without requiring proportionally larger imports from Earth.
\end{claim}

\begin{claim}[Repair before expansion]
No off-world factory should be scaled before it can inspect, maintain, and partially repair its own critical tools.
\end{claim}

\section{06 / Evidence program}

\subsection{Phase A: ground forge cell}
Build a small autonomous forge cell in a terrestrial laboratory. The cell receives standardized beams, nodes, fasteners, cables, and sensors; assembles a load-bearing lattice; inspects it; repairs a seeded defect; and releases a signed part passport.

\subsection{Phase B: hostile-environment analog}
Move the forge cell into thermal-vacuum, dust, lighting, communication-delay, and degraded-sensor conditions. The target is not flawless autonomy; it is graceful degradation with a complete failure ledger.

\subsection{Phase C: orbital warehouse demonstrator}
A small orbital hub stores modular elements, hosts mobile inspectors, and performs simple assembly and repair tasks. The exit criterion is a qualified structure assembled from at least three independently launched modules with local inspection and signed assurance.

\subsection{Phase D: lunar yard}
A lunar yard adds regolith handling, abrasive dust, day-night thermal extremes, local power constraints, and excavation. The first useful outputs should be boring: berms, pads, thermal shields, cable trays, spare brackets, and radiation mass. Civilization is made of boring things that do not fail.

\subsection{Phase E: asteroid and free-space industrialization}
Asteroids shift the architecture from surface construction to free-space material flow. Here StructureForge becomes an orbital ecology of miners, smelters, foundries, assembly yards, propellant depots, optics, mirrors, habitats, and beam arrays.

\section{07 / Constructor algebra}

\begin{speculative}
The future galactic factory is not an assembly line. It is a grammar that compiles intention into matter. In its mature form, StructureForge becomes a constructor algebra: a formal system whose terms are machines and whose reductions are safe physical transformations.
\end{speculative}

Let $\mathcal{C}$ be a category whose objects are certified material states and whose morphisms are qualified transformations:
\begin{equation}
    f: A \rightarrow B, \qquad f \in \mathrm{Hom}_{\mathcal{C}}(A,B).
\end{equation}
Composition $g\circ f$ is allowed only when physical interfaces, energy budgets, uncertainty, and assurance obligations compose:
\begin{equation}
    \mathsf{cert}(g\circ f) = \mathsf{cert}(g) \otimes \mathsf{cert}(f) \otimes \mathsf{cert}_{\mathrm{interface}}(A,B,C).
\end{equation}
A factory is then a theorem prover in matter: it proves that a desired object is reachable from available stocks under allowed transformations.

Define the \textit{industrial spell} as a tuple
\begin{equation}
    \Sigma = \langle D,\mathcal{S},\mathcal{T},\mathcal{E},\mathcal{W},\mathcal{A}\rangle,
\end{equation}
where $D$ is desire or design intent, $\mathcal{S}$ stock, $\mathcal{T}$ tools, $\mathcal{E}$ energy, $\mathcal{W}$ world constraints, and $\mathcal{A}$ assurance. The mystical word \textit{spell} is useful only if it remains operational: a spell is a reproducible transformation with known preconditions, known costs, and a signed trail.

\begin{hypothesis}[Self-reciting factory hypothesis]
A mature autonomous yard can store its own production grammar in the objects it produces, so that damaged or isolated fragments of the industrial network can reconstruct local capability from physical inscriptions, fiducials, and part passports.
\end{hypothesis}

This is not magic. It is a resilient encoding problem. The bridge to myth is that civilization has always hidden memory in objects: temples, tools, books, seeds, machines. StructureForge makes that memory executable.

\section{08 / Technology roadmap}

\begin{longtable}{p{0.18\linewidth}p{0.24\linewidth}p{0.46\linewidth}}
\toprule
\textbf{Horizon} & \textbf{Milestone} & \textbf{Exit criterion}\\
\midrule
0--12 months & Forge graph simulator & Typed process graph with risk-priced assembly planning and simulated assurance packages.\\
12--24 months & Ground robotic cell & Assembly, inspection, defect seeding, repair, and passport emission for simple lattice structures.\\
24--48 months & Thermal-vacuum/dust cell & Demonstrated degraded autonomy under hostile analog conditions with failure ledger.\\
48--72 months & Orbital warehouse demo & Multi-module assembly with local metrology and signed qualification.\\
72--120 months & Lunar yard pilot & Regolith-handling and locally useful construction products with measured import displacement.\\
120+ months & Positive closure loop & $\rho_F(T)>1$ for at least one critical infrastructure family.\\
\bottomrule
\end{longtable}

\section{09 / Failure modes}

\begin{itemize}
    \item \textbf{Interface sprawl.} Too many standards destroy robotic generality.
    \item \textbf{Autonomy theater.} A human-in-the-loop system is marketed as autonomous without delay-tolerant safety.
    \item \textbf{Evidence gap.} Parts are built but not qualified, making them unusable for critical infrastructure.
    \item \textbf{Dust and abrasion.} Lunar and asteroid materials break seals, bearings, optics, and connectors.
    \item \textbf{Thermal truth.} Structures assembled in benign conditions fail under actual thermal cycling.
    \item \textbf{Bootstrap illusion.} Local manufacturing consumes more imported tooling and consumables than it displaces.
\end{itemize}

\section{10 / Release}

The first release should include this source, PDF, bibliography, a forge-graph schema, a simple robotic assembly simulator, an example part passport, and an assurance checklist. StructureForge should be developed beside Orbis Edge-style latency-tolerant autonomy and artifact synchronization \cite{JMPOrbis2026}.

\input{bibliography.tex}
\end{document}
